;

; Android WinUsb driver installation.

;

[Version]

Signature           = "$Windows NT$"

Class               = AndroidUsbDeviceClass

ClassGuid           = {3F966BD9-FA04-4ec5-991C-D326973B5128}

Provider            = %ProviderName%

DriverVer           = 08/28/2014,11.0.0000.00000

CatalogFile.NTx86   = androidwinusb86.cat

CatalogFile.NTamd64 = androidwinusba64.cat



[ClassInstall32]

Addreg = AndroidWinUsbClassReg



[AndroidWinUsbClassReg]

HKR,,,0,%ClassName%

HKR,,Icon,,-1





[Manufacturer]

%ProviderName% = Google, NTx86, NTamd64





[Google.NTx86]



;Google Nexus One

%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_0D02

%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_0D02&MI_01

%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_4E11

%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4E12&MI_01



;Google Nexus S

%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_4E21

%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4E22&MI_01

%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_4E23

%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4E24&MI_01



;Google Nexus 7

%SingleBootLoaderInterface% = USB_Install, USB\VID_18D1&PID_4E40

%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4E42&MI_01

%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4E44&MI_01



;Google Nexus Q

%SingleBootLoaderInterface% = USB_Install, USB\VID_18D1&PID_2C10

%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_2C11



;Google Nexus (generic)

%SingleBootLoaderInterface% = USB_Install, USB\VID_18D1&PID_4EE0

%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4EE2&MI_01

%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4EE4&MI_02

%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4EE6&MI_01

%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4EE7

%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_D001



;Google Glass

%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_9001

%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_9001&MI_01



;Project Tango (generic)

%SingleBootLoaderInterface% = USB_Install, USB\VID_18D1&PID_4D00

%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4D02&MI_01

%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4D04&MI_02

%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4D06&MI_01

%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4D07





[Google.NTamd64]



;Google Nexus One

%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_0D02

%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_0D02&MI_01

%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_4E11

%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4E12&MI_01



;Google Nexus S

%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_4E21

%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4E22&MI_01

%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_4E23

%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4E24&MI_01



;Google Nexus 7

%SingleBootLoaderInterface% = USB_Install, USB\VID_18D1&PID_4E40

%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4E42&MI_01

%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4E44&MI_01



;Google Nexus Q

%SingleBootLoaderInterface% = USB_Install, USB\VID_18D1&PID_2C10

%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_2C11



;Google Nexus (generic)

%SingleBootLoaderInterface% = USB_Install, USB\VID_18D1&PID_4EE0

%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4EE2&MI_01

%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4EE4&MI_02

%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4EE6&MI_01

%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4EE7

%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_D001



;Google Glass

%SingleAdbInterface%        = USB_Install, USB\VID_18D1&PID_9001

%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_9001&MI_01



;Project Tango (generic)

%SingleBootLoaderInterface% = USB_Install, USB\VID_18D1&PID_4D00

%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4D02&MI_01

%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4D04&MI_02

%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4D06&MI_01

%CompositeAdbInterface%     = USB_Install, USB\VID_18D1&PID_4D07





[USB_Install]

Include = winusb.inf

Needs   = WINUSB.NT



[USB_Install.Services]

Include     = winusb.inf

AddService  = WinUSB,0x00000002,WinUSB_ServiceInstall



[WinUSB_ServiceInstall]

DisplayName     = %WinUSB_SvcDesc%

ServiceType     = 1

StartType       = 3

ErrorControl    = 1

ServiceBinary   = %12%\WinUSB.sys



[USB_Install.Wdf]

KmdfService = WINUSB, WinUSB_Install



[WinUSB_Install]

KmdfLibraryVersion  = 1.9



[USB_Install.HW]

AddReg  = Dev_AddReg



[Dev_AddReg]

HKR,,DeviceInterfaceGUIDs,0x10000,"{F72FE0D4-CBCB-407d-8814-9ED673D0DD6B}"



[USB_Install.CoInstallers]

AddReg    = CoInstallers_AddReg

CopyFiles = CoInstallers_CopyFiles



[CoInstallers_AddReg]

HKR,,CoInstallers32,0x00010000,"WdfCoInstaller01009.dll,WdfCoInstaller","WinUSBCoInstaller2.dll"



[CoInstallers_CopyFiles]

WinUSBCoInstaller2.dll

WdfCoInstaller01009.dll



[DestinationDirs]

CoInstallers_CopyFiles=11



[SourceDisksNames]

1 = %DISK_NAME%,,,\i386

2 = %DISK_NAME%,,,\amd64



[SourceDisksFiles.x86]

WinUSBCoInstaller2.dll  = 1

WdfCoInstaller01009.dll = 1



[SourceDisksFiles.amd64]

WinUSBCoInstaller2.dll  = 2

WdfCoInstaller01009.dll = 2



[Strings]

ProviderName                = "Google, Inc."

SingleAdbInterface          = "Android ADB Interface"

CompositeAdbInterface       = "Android Composite ADB Interface"

SingleBootLoaderInterface   = "Android Bootloader Interface"

WinUSB_SvcDesc              = "Android USB Driver"

DISK_NAME                   = "Android WinUsb installation disk"

ClassName                   = "Android Device"

